JULY 2017

|  |  |  |
| --- | --- | --- |
|  |  |  |

**Product Guide Specification**

Specifier Notes: This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on *MasterFormat 2016* and *The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy.*

The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code. Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement. Coordinate this section with other specification sections and the Drawings. Delete all “Specifier Notes” after editing this section.

**Section 28 00 00: Electronic Safety and Security**

**Section 28 05 00: Common Work Results For Electronic Safety and Security**

**Section 28 05 19.11: Digital Video Recorders**

**PENTA-BRID 4K DVR - 16-CHANNEL 2U HDCVI DIGITAL VIDEO RECORDER**

1. **– GENERAL**
	1. SUMMARY
		1. Section Includes
			1. Section 28 05 23: Storage Area Network Electronic Safety and Security
			2. Section 28 05 25: Cloud Based Storage for Electronic Safety and Security
			3. Section 28 05 29: Storage Management Software for Electronic Safety and Security
			4. Section 28 05 31: Communications Equipment for Electronic Safety and Security
		2. Related Sections
			1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].

\*\*\*\*\*\*\*\*\*\*Specifier’s note: Include those standards referenced elsewhere in this SECTION.

* 1. REFERENCES
		1. Federal Communications Commission (FCC) ([www.fcc.gov](http://www.fcc.gov))
			1. CFR 47 FCC Part 15 Subpart B
		2. Underwriters Laboratories, Inc. (UL) (www.ul.com)
			1. Conforms to UL safety standards
	2. SYSTEM DESCRIPTION
		1. Section Includes
			1. Digital Video Recorders
		2. Performance Requirements
			1. The Penta-brid 4K DVR shall be an embedded processer with embedded Linux operating system to record video from HDCVI, AHD, TVI, CVBS, and IP data sources.
			2. The Penta-brid 4K DVR shall be capable of storing up to 24 TB of data from 16 analog camera inputs and 48 IP camera video inputs with up to 12 MP resolution for each IP input.
			3. The Penta-brid 4K DVR shall use the Smart H.264+, H.264, and MJPEG Video compression protocols.
			4. The Penta-brid 4K DVR shall have a maximum incoming bandwidth of 256 Mbps and 384 Mbps forwarding bandwidth.
			5. The Penta-brid 4K DVR shall automatically detect and recognize the transmission protocol (HDCVI, AHD, TVI or CVBS) of each attached analog camera.
			6. The Penta-brid 4K DVR shall offer a selection of built-in recording options and schedules.
			7. The Penta-brid 4K DVR shall offer a smart search function to search a specific region of the playback video.
			8. The Penta-brid 4K DVR shall come in a 2U-high casing.
	3. SUBMITTALS

* + 1. Submit under provisions of Section [01 33 00.]
		2. Product Data:
			1. Manufacturer’s data, user and installation manuals for all equipment and software programs including computer equipment and other equipment required for complete video management system.
		3. Dimensional Drawings; include
			1. Overall device dimensions.
			2. Dimensions specific for installation.
		4. Closeout Submittals
			1. User manual.
			2. Parts list.
			3. Maintenance requirements.
	1. QUALITY ASSURANCE
		1. Manufacturer:
			1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.
		2. Video Surveillance System:
			1. List certifying bodies (UL, CSA, etc.)
			2. Provide evidence of compliance upon request.
		3. Installer:
			1. Minimum of [5] years of experience installing Video Surveillance System.
	2. DELIVERY, STORAGE AND HANDLING
		1. Comply with requirements of Section 01 60 00.
		2. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels.
		3. Protect store materials from environmental and temperature conditions following manufacturer’s instructions.
		4. Handle and operate products and systems according to manufacturer’s instructions.
	3. WARRANTY
		1. Provide manufacturer’s warranty covering [2] years for replacement and repair of defective equipment. Warranty varies country to country.
	4. MAINTENANCE
		1. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.
		2. Provide factory direct technical support via phone and e-mail.
1. **– PRODUCTS**
	1. MANUFACTURERS
		1. [Acceptable Manufacturer:

Dahua Technology USA Inc.

23 Hubble, Irvine, CA 92618

Tel: (949) 679-7777

Fax: (949) 679-5760

Email: sales.usa@global.dahuatech.com]

* + 1. Substitutions: [Not permitted.] [Under provisions of Division 1.]
			1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
			2. [Proposed substitutions must provide a line-by-line compliance documentation.]
	1. PENTA-BRID 4K DVR - 16-CHANNEL 2U DIGITAL VIDEO RECORDER
	[X58A3S]

		1. General Characteristics:
			1. The Penta-brid 4K DVR shall be an embedded processer with embedded Linux operating system to record video from HDCVI, AHD, TVI, CVBS, and IP data sources.
			2. The Penta-brid 4K DVR shall be capable of storing up to 24 TB of data from 16 analog camera inputs and 48 IP camera video inputs with up to 12 MP resolution for each IP input.
			3. The Penta-brid 4K DVR shall use the Smart H.264+, H.264, and MJPEG video compression protocols.
			4. The Penta-brid 4K DVR shall have a maximum incoming bandwidth of 256 Mbps and 384 Mbps forwarding bandwidth.
			5. The Penta-brid 4K DVR shall automatically detect and recognize the transmission protocol (HDCVI, AHD, TVI or CVBS) of each attached analog camera.
			6. The Penta-brid 4K DVR shall offer a selection of built-in recording options and schedules.
			7. The Penta-brid 4K DVR shall be powered by a 100 to 240 VAC, 50/60 Hz power supply and consume less than 40 W of power.
		2. Display
			1. The Penta-brid 4K DVR shall offer two (2) HDMI, one (1) VGA, and one (1) TV interface. The HDMI 1 port shall provide output up to 4K and 2K.
			2. The Penta-brid 4K DVR shall offer display resolutions of: 3480 x 2160,
			2560 x 1440 1920 × 1080, 1280 × 1024, 1280 × 720, and 1024 × 768.
			3. The Penta-brid 4K DVR shall offer 1/4/8/9/16/25/36 multi-screen display.
			4. The Penta-brid 4K DVR shall offer four (4) rectangular privacy mask zones for each camera.
			5. The Penta-brid 4K DVR shall offer an on-screen display that lists the camera title, time, video loss indication, camera lock indication, motion detection, and recording indicator.
		3. Video Detection and Alarm
			1. The Penta-brid 4K DVR shall offer the following trigger events: recording, PTZ, tour, alarm our, video push, Email, FTP, snapshot, buzzer, and screen tips.
			2. The Penta-brid 4K DVR shall be capable of detecting motion (396 zones), video loss, tampering, and diagnosis.
			3. The Penta-brid 4K DVR shall offer 16 alarm inputs and six (6) relay outputs.
		4. Interface
			1. The Penta-brid 4K DVR shall have 16 analog (HDCVI, AHD, TVI or CVBS) camera inputs and 48 IP camera video inputs.
			2. The Penta-brid 4K DVR shall allow all 64 (16 analog plus 48 IP) video channels to record IP cameras.
			3. The Penta-brid 4K DVR shall offer two (2) USB 2.0 auxiliary ports and two (2) USB 3.0 auxiliary ports.
			4. The Penta-brid 4K DVR shall offer one serial interface that connects to one (1) of the following protocols:
				1. RS232: for PC communication or keyboard control
				2. RS22/RS485: for PTZ control.
				3. RS485
			5. The Penta-brid 4K DVR shall offer 16 audio input channels and one (1) audio output channel.
			6. The Penta-brid 4K DVR shall allow two-way talk with one (1) BNC microphone input connector and one (1) BNC microphone output connector.
			7. The Penta-brid 4K DVR shall offer 8 or 16 loop-out BNC connectors for the HDCVI and the CVBS protocols.
		5. Storage
			1. The Penta-brid 4K DVR shall come with eight (8) SATA ports that can each support an 8 TB HDD.
			2. The Penta-brid 4K DVR shall support one (1) eSATA port.
		6. Playback and Backup
			1. The Penta-brid 4K DVR shall support output to 1/4/9/16 playback devices.
			2. The Penta-brid 4K DVR shall allow recorded video searches by time/date, motion detection event, Exact Search, and Smart Search.
			3. The Penta-brid 4K DVR shall offer the following playback functions: Play, Pause, Stop, Rewind, Fast Play, Slow Play, Next File, Previous File, Next Camera, Previous Camera, Full Screen, Repeat, Shuffle, Backup Selection, and Digital Zoom.
			4. The Penta-brid 4K DVR shall allow data backup via a USB device or another network.
		7. Recording
			1. The Penta-brid 4K DVR shall employ the Smart H.264+, H.264, and the MJPEG video compression protocols.
			2. The Penta-brid 4K DVR shall offer video recording resolutions of 4K, 4 MP, 1080p, 720p, 960H, D1, HD1, BCIF, CIF, and QCIF.
			3. The Penta-brid 4K DVR shall allow a bit rate of 1 Kbps to 12288 Kbps per channel.
			4. The Penta-brid 4K DVR shall offer dual recording at the following rates:
				1. Main Stream:

CVI/AHD:

1st and 9th channels: 4K or 4 MP at 15 fps

Other Channels:
4 MP at 15 fps,
1080p, 720p, 960H, D1, HD1, BCIF, CIF, QCIF at 30 fps

* + - * 1. Sub Stream: 960H, D1, CIF, QCIF at 30 fps
			1. The Penta-brid 4K DVR shall offer the following built-in recording modes:
				1. Manual
				2. Schedule, regular or continuous
				3. Video Detection: Motion Detection, Video Loss, Tampering
				4. Alarm
				5. Stop
			2. The Penta-brid 4K DVR shall offer a recording interval between 1 minute and 60 minutes. In addition, The Penta-brid 4K DVR shall offer a pre-record interval of between 1 second to 30 seconds, and a post-record interval of between 10 seconds to 300 seconds.
			3. The Penta-brid 4K DVR shall be capable of recording from third-party devices, including: Dahua, Arecont Vision, AXIS, Bosch, Brickcom, Canon, CP Plus, Dynacolor, Honeywell, Panasonic, Pelco, Samsung, Sanyo, Sony, Videotec, and Vivotek.
		1. IP Connectivity
			1. The Penta-brid 4K DVR shall allow full control and configuration capabilities via a TCP/IP network.
			2. The Penta-brid 4K DVR shall offer two RJ-45 ports (1000 Mbps).
			3. The Penta-brid 4K DVR shall support a maximum of 128 user access points.
			4. The Penta-brid 4K DVR shall conform to the ONVIF 2.41 and to the CGI standard.
			5. The Penta-brid 4K DVR shall support the IPv6 internet-layer protocol for packet switched internetworking across multiple IP networks.
			6. The Penta-brid 4K DVR shall support the IPv4/ IPv6, HTTP, HTTPS, SSL, TCP/IP, UDP, UPnP, ICMP, IGMP, SNMP, RTSP, RTP, SMTP, NTP, DHCP, DNS, PPPOE, DDNS, FTP, IP Filter, QoS, Bonjour, and 802.1x.
			7. The Penta-brid 4K DVR shall support the IOS and the Android mobile operating systems.
		2. Intelligent Video System
			1. The Penta-brid 4K DVR shall offer a built-in Intelligent Video System to provide advanced analytics for a scene transmitted from a camera connected to the DVR.
			2. The Intelligent Video System shall offer intelligent video analytics built-in to The Penta-brid 4K DVR.
			3. The Intelligent Video System shall be capable of processing and analyzing video within the camera itself, with no extra hardware required.
			4. The Intelligent Video System shall trigger an alarm and take a defined action for the following events:
				1. Standard Features

Tampering with the camera.

Error writing to an onboard Micro SD Card.

Error sending or receiving data over the network.

Unauthorized access to the camera.

* + - * 1. Premium Features

Motion: object moves through any part of the scene.

Tripwire: a target crosses a user-defined line.

Intrusion: a target enters or exits a defined perimeter.

Scene Change: a person or object moves the camera to change the scene or covers the camera to obscure the scene.

Abandoned/Missing Object: a target leaves an object in a designated area, or a target removes and object from the same designated area.

* + - * 1. Advanced Features

Facial Detection: detects and captures a snapshot of a human face in a defined area within a scene.

People Counting: Measure the number of customers, visitors or passengers in a surveillance scene.

* + - 1. The Intelligent Video System features are available on the following channels:
				1. Standard are Premium features shall be available on up to six (6) channels.
				2. The People Counting feature shall be available on one channel.
				3. The Facial Detection feature without the people counting feature in use shall be available on:

With HDMI-2 Port not in use: four (4) channels

With HDMI-2 Port in use: two (2) channels

* + - * 1. The Facial Detection feature with the people counting feature in use shall be available on:

With HDMI-2 Port not in use: three (3) channels

With HDMI-2 Port in use: one (1) channel

* + 1. Installation Requirements
			1. The Penta-brid 4K DVR shall be capable of operating in temperatures between -10°C to +55°C (+14°F to +131°F).
			2. The Penta-brid 4K DVR shall receive power from a 100 to 240 VAC, 50/60 Hz power source and consume less than 40 W of power.
1. **– EXECUTION**
	1. EXAMINATION
		1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
		2. Do not begin installation until unacceptable conditions are corrected.
	2. PREPARATION
		1. Protect devices from damage during construction.
	3. INSTALLATION
		1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
		2. Perform installation with qualified service personnel.
		3. Install devices in accordance with the National Electrical Code or applicable local codes.
		4. Ensure selected location is secure and offers protection from accidental damage.
		5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
	4. FIELD QUALITY CONTROL
		1. Test snugness of mounting screws of all installed equipment.
		2. Test proper operation of all video system devices.
		3. Determine and report all problems to the manufacturer’s customer service department.
	5. ADJUSTING
		1. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
		2. Make any adjustment of camera settings to comply with specific customer’s need.
	6. DEMOSTRATION
		1. Demonstrate at final inspection that video management system and devices functions properly.

END OF SECTION